//Verison=2.2
//Example,Don't Delete flowing text!
//Button NIMI // Generator NIMI 
//Button NIMI 100 // Generator NIMI and Delay 100ms, 100 not is nessary
//Button INT0 // Generator INT0 and Delay 200ms
//Button RESETAMBE3000
//Button RESET3252
//Send 1 command, Receive 2 response with one is not verify.
//Command ID: CARRIER_LOST // necessary!
//Summary  // not essential, 
//Send command: 61 00 02 00 19 00 // necessary!
//Pause=300 // not essential, unit: ms; Pause 300ms after Send command
//Timeout=100 // not essential, unit: ms; if not receive '84 A9 61 ...' in 100ms after send command, Timeout error will happen!
//*Receive Data: 61 00 02 51 19 00 // not essential, receive but not verify
//Receive Data: 61 00 02 51 19 20 // not essential, receive and verify 
//.Set x = AA B0  -- Define var x ; Added in ver2.2
// ... 61 00 02 00 19 {x}   --- use the defined var, The {x} will be replaced with AA B0 
//

//BASE_SET    tsinghua set 01 ambe set +2c 03 st24set 06 ambe 3000 set 00 
.Set READY_VAR = 01
.Set VOCODER_VAR = 03

//Vocoder Auto selection
//.Set VOCODER_VAR = ff

//Call match test  
//.Set READY_VAR = 05

//Voice call with 19 02, and Mod_Gain inverted
//.Set READY_VAR = 02





Command ID:	VOCODER_SEL
Send	Command: 84 A9 61 00 02 00 10 {VOCODER_VAR}
Receive	Command:84 A9 61 00 02 00 10 00
Pause 3000

Command ID:	DPMR_CC
Send	Command: 84 A9 61 00 04 03 5C ff 5d 7f
Receive	Command:84 A9 61 00 02 03 5C 00
Command ID: WORK_MODE
Send command: 84 A9 61 00 04 00 18 01 00 00
Receive Data: 84 A9 61 00 02 00 18 00
Command ID: PROCESS_MODE
Send command: 84 A9 61 00 02 00 1A 83
Receive Data: 84 A9 61 00 02 00 1A 00
Command ID:	ADDRESSING_MODE
Send	Command: 84 A9 61 00 02 03 28 01
Receive	Command:84 A9 61 00 02 03 28 00


Command ID: REPORT_FIELD
Send command: 84 A9 61 00 02 00 1D ff
//Send command: 84 A9 61 00 01 00 1D 00
Receive Data: 84 A9 61 00 02 00 1D 00
Command ID: DPMR_OWN_ID
Send command: 84 A9 61 00 04 03 51 12 34 56
Receive Data: 84 A9 61 00 02 03 51 00
Command ID:	DEMOD_GAIN
Send	Command: 84 A9 61 00 03 00 1C 00 00
Receive	Command:84 A9 61 00 02 00 1C 00
Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY  1847 set 01 3700 set 02
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
